{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":14,"rows_kept":18,"flags":["formulas_cached_only"]}
["Design Table for: Terminal Lug"]
[null,"$COMMENT","$DESCRIPTION","$PARTNUMBER","$COLOR","Thickness@Sheet-Metal","$VALUE@Tongue Material Thickness@Equations","$VALUE@Stud Size@Equations","$VALUE@Tongue Width@Equations","$VALUE@C@Equations","$VALUE@E Max.@Equations","$VALUE@L Max.@Equations","$VALUE@Wire Size Max (cmil)@Equations","$VALUE@Hole Diameter@Equations"]
["M6 - 33100","Lug - Stud M6, Wire max 33100 circular mils (16mm2)","Lug - Stud M6, Wire 33100 cmil","$C",9871014,1.52,"=1.52","=6mm","=11.89mm'W","=13.49mm","=23.65mm","=29.67mm","=33100'in circular mils","=3.7"]
["M8 - 33100","Lug - Stud M8, Wire max 33100 circular mils (16mm2)","Lug - Stud M8, Wire 33100 cmil","$C",9871014,1.52,"=1.52","=8mm","=15.88mm'W","=13.49mm","=23.65mm","=31.65mm","=33100'in circular mils","=3.7"]
["M6 - 20800","Lug - Stud M6, Wire max 20800 circular mils (10.5mm2)","Lug - Stud M6, Wire 20800 cmil","$C",9871014,1.3,"=1.3","=6mm","=11.91mm'W","=9.12mm","=17.68mm","=23.70mm","=20800'in circular mils","=3.7"]
["M8 - 20800","Lug - Stud M8, Wire max 20800 circular mils (10.5mm2)","Lug - Stud M8, Wire 20800 cmil","$C",9871014,1.3,"=1.3","=8mm","=14.27mm'W","=10.31mm","=20.07mm","=27.28mm","=20800'in circular mils","=3.7"]
["M4 - 20800","Lug - Stud M4, Wire max 20800 circular mils (10.5mm2)","Lug - Stud M4, Wire 20800 cmil","$C",9871014,1.3,"=1.3","=4mm","=10.31mm'W","=9.12mm","=18.87mm","=24.10mm","=20800'in circular mils","=3.7"]
["M3.5 - 13100","Lug - Stud M3.5, Wire max 13100 circular mils (6.64mm2)","Lug - Stud M3.5, Wire 13100 cmil","$C",9871014,1.07,"=1.07","=3.5mm","=9.53mm'W","=7.67mm","=14.61mm","=19.43mm","=13100'in circular mils","=3.7"]
["M4 - 13100","Lug - Stud M4, Wire max 13100 circular mils (6.64mm2)","Lug - Stud M4, Wire 13100 cmil","$C",9871014,1.07,"=1.07","=4mm","=9.53mm'W","=7.67mm","=14.61mm","=19.43mm","=13100'in circular mils","=3.7"]
["M6 - 13100","Lug - Stud M6, Wire max 13100 circular mils (6.64mm2)","Lug - Stud M6, Wire 13100 cmil","$C",9871014,1.07,"=1.07","=6mm","=13.49mm'W","=11.89mm","=18.69mm","=25.50mm","=13100'in circular mils","=3.7"]
["M8 - 13100","Lug - Stud M8, Wire max 13100 circular mils (6.64mm2)","Lug - Stud M8, Wire 13100 cmil","$C",9871014,1.07,"=1.07","=8mm","=13.49mm'W","=11.89mm","=18.69mm","=25.50mm","=13100'in circular mils","=3.7"]
["M3.5 - 05180","Lug - Stud M3.5, Wire max 5180 circular mils (2.62mm2)","Lug - Stud M3.5, Wire 5180 cmil","$C",9871014,0.84,"=0.84","=3.5mm","=8.71mm'W","=7.14mm","=11.73mm","=16.15mm","=5180'in circular mils","=3.7"]
["M3.5 - 05180 (2)","Lug - Stud M3.5, Wire max 5180 circular mils (2.62mm2)","Lug - Stud M3.5, Wire 5180 cmil","$C",9871014,0.84,"=0.84","=3.5mm","=6.35mm'W","=4.34mm","=8.94mm","=12.19mm","=5180'in circular mils","=3.7"]
["M4 - 05180","Lug - Stud M4, Wire max 5180 circular mils (2.62mm2)","Lug - Stud M4, Wire 5180 cmil","$C",9871014,0.84,"=0.84","=4mm","=8.71mm'W","=7.14mm","=11.73mm","=16.15mm","=5180'in circular mils","=3.7"]
["M6 - 05180","Lug - Stud M6, Wire max 5180 circular mils (2.62mm2)","Lug - Stud M6, Wire 5180 cmil","$C",9871014,0.84,"=0.84","=6mm","=11.91mm'W","=11.10mm","=15.70mm","=21.72mm","=5180'in circular mils","=3.7"]
["M3.5 - 03260","Lug - Stud M3.5, Wire max 3260 circular mils (1.65mm2)","Lug - Stud M3.5, Wire 3260 cmil","$C",9871014,0.84,"=0.84","=3.5mm","=5.54mm'W","=3.96mm","=8.56mm","=11.40mm","=3260'in circular mils","=3.7"]
["M3.5 - 03260 (2)","Lug - Stud M3.5, Wire max 3260 circular mils (1.65mm2)","Lug - Stud M3.5, Wire 3260 cmil","$C",9871014,0.84,"=0.84","=3.5mm","=7.14mm'W","=6.35mm","=11.07mm","=14.58mm","=3260'in circular mils","=3.7"]
["M4 - 03260","Lug - Stud M4, Wire max 3260 circular mils (1.65mm2)","Lug - Stud M4, Wire 3260 cmil","$C",9871014,0.84,"=0.84","=4mm","=7.14mm'W","=6.35mm","=11.07mm","=14.58mm","=3260'in circular mils","=3.7"]